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. ADR PLACARDING GUIDE
LU EYZETO BRI \EnicLES CARRYING PACKAGES

ADR IMDG IATA DGSA A clear guide to when orange plates and hazard placards
are required for road transport under ADR.
KEY POINTS

This guide is for vehicles carrying dangerous goods For most other classes (2, 3, 4, 5, 6, 8 and 9) carried

in packages (e.g. boxes, drums, IBCs, etc.). in packages, the vehicle does not normally require

Orange plates (plain, without numbers) are required hazard placards.

at the front and rear of the vehicle when carrying Only one orange plate is required at the front and one

dangerous goods subject to full ADR. at the rear.

Hazard placards (diamonds) are only required on the Placards and plates must be clearly visible, correctly

vehicle for Class 1 (explosives) and Class 7 positioned and not obscured.

(radioactive materials), except where specific Exemytions may apply (e.g. limited quantities, excepted

exceptions apply. quantities or ADR 1.1.3.6). Always check the applicable
provisions.

PACKAGED DANGEROUS GOODS - CLASSES 2, 3, 4, 5, 6, 8 AND 9
(No vehicle hazard placards normally required)

Orange plates at the front
and rear of the vehicle
(plain, without numbers).

No hazard diamond placards
on the vehicle for packages
in these classes (unless a
specific provision requires

otherwise).
AppliesoHingle and Front view Side view Rear view
§ (one orange plate) (no vehicle placards) (one orange plate)
{ ) (BOTH sides of vehicle) ; e pite)

CLASS 1 - EXPLOSIVES (IN PACKAGES)
(Vehicle hazard placards required, except Division 1.4, Compatibility Group S)

Orange plates at the front
and rear of the vehicle
(plain, without numbers).

Class 1 hazard placards on
both sides and at the rear
of the vehicle.
Exception: Division 1.4,
Compatibility Group S does
not require Class 1 vehicle
placards, and orange plates
are not automatically required.
Check applicable provisions.

Front view Side view
(one orange plate) (Class 1 placard) (one orange plate +
(BOTH sides of vehicle) Class 1 placard)

CLASS 7 - RADIOACTIVE MATERIALS (IN PACKAGES)
(Vehicle hazard placards required, except for excepted packages)

Orange plates at the front
and rear of the vehicle

(plain, without numbers)
Class 7 hazard placards on
both sides and at the rear

of the vehicle.

Exception: Excepted packages
do not require vehicle placards
or orange plates.

Note: For exclusive-use
consignments with a single
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UN numer, umbered orange Bottica Side view Rear view
plates (with the UN number (Class Ziplacand]
and hazard identification number) ~(One orange plate) (Bo(ma:if,esp;?eh?de, {one gfody piste ¢
may be required instead of plain | Class 7 placard)
orange plates. Check ADR 5.3.2.1.4 and 5.3.2.1.6.

REGULATORY REFERENCES PLEASE NOTE

ADR 5.3.1.5 - Placarding of vehicles This s a general guide for information purposes only.

ADR 5.3.2.1.1 - Orange plates (front and rear) Always check the full ADR requirements and any applicable

ADR 5.3.2.1.4 - Radioactive material (exclusive use) exemptions or special provisions for your specific consignment.

ADR 5.3.2.1.6 - Alternative placarding provisions





